Zero-Touch WebEx Calling CUBE configuration

This script extracts WxC SIP Trunk configuration from a CSV file, connects to the CUBE and configure WxC SIP trunk tenant , dial peers and translations on the CUBE. It relies on a configuration template that can be changed to integrate with any SIP/PSTN provider if needed.

